**Winterizing**

|  |  |
| --- | --- |
| Inboard Gas Engines up to 4 cylinders | $101.00 |
| Inboard Gas Engines-6 and 8 cylinders | $145.00 |
| Out drives - Sail drive – V drive – Jet drive | $70.00 |
| Inboard Diesel Engines 1 and 2 cylinder | $100.00 |
| Inboard Diesel Engines 3 and 4 cylinder | $130.00 |
| Inboard Diesel Engines 6 cylinder | $155.00 |
| Larger Diesel Engines | Hourly rate |
| Generator-Gas or Diesel | $116.00 |
| Removal of Out drives, check alignment,  Grease universal joint and re-install | Hourly Rate |
| Batteries removed,  Stored and charged (each) | $40.00 |
| Batteries removed for owner (each) | $28.00 |
| Batteries charged and unhooked | $33.00 |

**MUFFLERS REQUIRING DRAINAGE + $14.00**

**Note**: **All materials for winterizing are additional**; materials for removal of out drives are additional. Winterizing includes fogging the motor, removal of hoses and water plugs and adding nontoxic anti-freeze.